English
Update FBs-30GM’s kernel:

1. Prepare a USB flash drive preformatted with the FAT32 file system.
2. Create a file named “Setting0.ini” with the content below 
(take kernel update file named “package_21c6e243.zip” as example) 
and put this file in your USB root directory. 

ACTION=SW_INSTALL
PARAMETER=package_21c6e243.zip

3. Insert the USB flash drive containing “Setting0.ini” to FBs-30GM.
4. Turn off FBs-30GM and on again, wait until RUN led is yellow: it means the system has finished restarting.
5. Pull out the USB and check its root directory. If a file named “Setting0.out” exists, 
   it means that the kernel has been changed successfully.




繁體中文
1.確認USB隨身碟的根目錄裡沒有setting0.out的檔案, 若已存在setting0.out的檔案,
  則setting0.ini這兩個檔案要放在USB的根目錄裡, 再把USB插上30GM, 把30GM重新開機直到系統就緒就安裝結束了

2.安裝完成後可以看到USB裡出現一個setting0.out的檔案, 代表已經成功安裝